



Firmware file is ai03\_orbit\_x\_via.hex

Install instructions:

1. If computer does not have drivers for atmega32u4:
   1. Open qmk\_toolbox.exe
   2. When QMK toolbox asks to install drivers, select Yes.  
      
   3. The drivers will install slowly.  
      
   4. Restart computer to finish driver install.
2. After drivers are installed, open qmk\_toolbox.exe.
3. Click the Open button under “Local File”, and select the firmware file ai03\_orbit\_x\_via.hex.  
   /
4. Select atmega32u4 for Microcontroller, and turn on “Flash when ready”.  
   
5. Connect the PCB. Firmware will automatically flash, and the device will appear as “ai03 Design Studio OrbitX” after success.